**OSHA-Required Work Practices for Lead Construction**

**Maximum Exposure Level Required Action**

**(ug/m3)** l

l

l

l Protective Clothing (change daily)

l

**200** ---- l

l

l Exposure monitoring (quarterly)

l Respirator

l Protective clothing (Change weekly)

l Separate change area

l Separate clothing disposal container

l Prohibited activities

l Showers

l Eating facility

l Signage

l Written compliance program

l

l

**PEL / 8 Hr** **50** ----- l

l

l Exposure monitoring (semiannual)

l Annual Training

l Biological monitoring (BLL/ZPP)

l Medical Surveillance (30-day exposure)

l

l

**Action Level** **30** ----- l

l

l Awareness training

l Engineering & work practice controls

l Housekeeping requirements

l Handwashing facilities

l Recordkeeping

l

***Any* disturbance** -------- l

l

l

**OSHA 29 CFR 1926.62 Lead Standard**

8-hour time-weighted average action level (AL): 30 ug/m3

8-hour time-weighted permissible exposure limit (PEL): 50 ug/m3