**OSHA-Required Work Practices for Lead Construction**

**Maximum Exposure Level Required Action**

 **(ug/m3)** l

l

l

 l Protective Clothing (change daily)

 l

 **200** ---- l

 l

 l Exposure monitoring (quarterly)

 l Respirator

 l Protective clothing (Change weekly)

 l Separate change area

 l Separate clothing disposal container

 l Prohibited activities

 l Showers

 l Eating facility

 l Signage

 l Written compliance program

 l

 l

 **PEL / 8 Hr** **50** ----- l

 l

 l Exposure monitoring (semiannual)

 l Annual Training

 l Biological monitoring (BLL/ZPP)

 l Medical Surveillance (30-day exposure)

 l

 l

 **Action Level** **30** ----- l

 l

 l Awareness training

 l Engineering & work practice controls

 l Housekeeping requirements

 l Handwashing facilities

 l Recordkeeping

 l

 ***Any* disturbance** -------- l

l

 l

**OSHA 29 CFR 1926.62 Lead Standard**

8-hour time-weighted average action level (AL): 30 ug/m3

8-hour time-weighted permissible exposure limit (PEL): 50 ug/m3